

|  |  |  |
| --- | --- | --- |
| **CREMATION MACHINE QUOTATION SHEET** | | |
|  | ITEM NO | ADIKRS3000-061 |
| FOB QINGDAO | USD99,500.00 |
| 40'OT container | 1PCS |
| OUT DIMENSION | 4100\*2100\*2300MM |
| INNER CHAMBER SIZE | 700\*700\*2200MM |
| G.W | 13.5T |
| OIL CONSUMPTION | 30-40L/H |
| CREMATION TIME | 40-70MINUTES PER BODY |
| TOTAL POWER | 18KW |
| WORKING TEMPERATURE | 700-900℃ |
| BURNING FUEL | diesel or the LPG,LNG for choose |
| WORKING VOLTAGE AND FREQUENCY | 380V,50HZ or 110V-220V,,60HZ,could  choose the one used in your place |
| MATERIAL AND THE PART FEATURE | The inside of this pick ashes cremation machine adopt GB standard proximate material combining new refractory materials, appearance made of quality stainless steel material package,equipped with the lifting cart,lift cooling  cover,main combustion chamber,seconary combustion chamber,oven door system,flue system,oil supply system,air supply system,induced draught system, and the electric control system. |
| warranty | 1.electric appliance:1 year 2.bed surface:500corpys 3.heart:2 years   1. burner:2 years 2. control system:2 years |
| **The feature of this cremation machine**  **1.the structure feature:** | | |

# the machine finish the whole installation at plant and export directly ,no need the assembling in work place.could use directly on plat floor.

**2.electric material:**

**mainly use the imported kind to make sure the longer life and the easy change for maintain if in need.**

1. thermal insulation properties

adopt the newest thermal insulation material, good insulation effect, long life,no moving,no damage and no subside during the transportation.

1. electric control system

the operation system adopt the CNC touch screen,nice looking,easy operate,and advanced,also prepare the traditional switching control mode to keep the stabality of the machine.

MOQ:one set

Payment terms:50%TT in advance,50%TT before shipment Delivery Time:as quantity,common is 30 days more or less. The quotation is valid in one month